RISK ASSESSMENT: 
TYPE: WORKPLACE 

Assessment Title: 
Garage
Assessed By: 
Harwood H&S Portal
Date of Assessment: 
9th August 2026

This template applies if employees: 
· Work is carried out in a vehicle garage, workshop or repair facility
· Employees inspect, service, maintain or repair vehicles
· Vehicles are moved, lifted or worked on within the premises
· Employees use vehicle lifts, tools, machinery or workshop equipment
· Employees handle fuels, oils, chemicals, batteries or other hazardous substances
· Work involves welding, grinding, hot work or other activities that may create additional hazards
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IMPORTANT:

This risk assessment template is provided by the Harwood Health & Safety Portal as a general guide only. It must be reviewed and adapted to reflect your specific workplace, activities, hazards and control measures. 
Using this template without appropriate review and customisation does not constitute a suitable and sufficient risk assessment.



HOW TO USE THIS RISK ASSESSMENT
1) Identify the hazards – look at the task, activity or workplace and identify anything that could cause harm 
2) Identify who might be harmed and how – consider employees, contractors, visitors and anyone else who could be affected
3) Establish what harm could occur – describe potential injuries or incidents 
4) Record existing controls – list the control measures already in place to reduce the risk 
5) Calculate the risk - use the risk rating matrix to determine the risk rating (likelihood x severity)
6) Decide on further controls – determine what additional activities are needed to reduce the risk further 
7) Assign responsibility – name the person or job role responsible for implementing the additional controls 
8) Set a date – create a target for when the additional controls need to be put into place 
9) Record the residual risk rating – reassess the risk after implementing further controls
10) Review and update – review this assessment regularly and when there are changes to keep it accurate and up to date 





	
1. 
	WHAT IS THE HAZARD?
	Slips, Trips & Falls

	
	Describe what could cause harm
	Oil, fuel, water, tools, vehicle parts, cables or other materials creating slippery or obstructed floors and walkways within the garage



	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Delivery drivers
· Customers and visitors



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Slips, trips and falls
· Sprains and strains
· Cuts and bruising
· Fractures
· Head injuries



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Floors and walkways are kept reasonably clear
· Oil, fuel and other spills are dealt with promptly
· Waste, parts and tools are removed from work areas regularly
· Cables and hoses are positioned to minimise trip hazards
· Suitable spill kits are available
· Materials and equipment are stored safely
· Adequate lighting is provided
· Suitable footwear is worn where required

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	3
	3
	9 – MEDIUM 



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Carry out regular housekeeping inspections
· Improve arrangements for dealing with spills and waste
· Keep vehicle access and pedestrian routes clear
· Review recurring slip or trip hazards and introduce additional controls

	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 



	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	3
	6 - MEDIUM

	
1. 
	WHAT IS THE HAZARD?
	Vehicle Movement & Workplace Transport

	
	Describe what could cause harm
	Vehicles being driven, manoeuvred or parked within the garage, workshop or surrounding yard

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Vehicle operators
· Contractors
· Customers and visitors



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Being struck or run over
· Crushing or trapping injuries
· Collision injuries
· Fractures or other serious injuries
· Serious or fatal injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Vehicle routes and pedestrian areas are clearly defined
· Vehicle movements are controlled within the workshop
· Suitable speed limits are established
· Drivers are authorised and competent
· Vehicles are secured when stationary
· Reversing is avoided where reasonably practicable
· Suitable visibility aids or assistance are used where required
· Pedestrian access is restricted from vehicle work areas where appropriate
· Adequate lighting is provided

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review vehicle and pedestrian routes regularly
· Improve segregation where vehicle and pedestrian movements overlap
· Review reversing arrangements
· Reinforce workshop traffic rules where unsafe practices are identified



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE

	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW



	
1. 
	WHAT IS THE HAZARD?
	Vehicle Lifting & Working Under Vehicles

	
	Describe what could cause harm
	Vehicles being raised on vehicle lifts, jacks or ramps, including work carried out underneath raised vehicles

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Vehicle collapse or falling from lifting equipment
· Crushing or trapping injuries
· Serious fractures
· Head injuries
· Serious or fatal injury

	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Vehicle lifts and lifting equipment are suitable for the vehicles being worked on
· Lifting equipment is inspected and maintained appropriately
· Only trained and competent employees operate vehicle lifts
· Vehicles are positioned correctly before lifting
· Manufacturer instructions and safe operating procedures are followed
· Vehicles are secured before work begins underneath
· Suitable axle stands or additional supports are used where required
· Employees are kept clear while vehicles are being raised or lowered
· Defective lifting equipment is removed from use

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM 

	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Ensure lifting equipment receives appropriate thorough examination and inspection
· Check vehicle weight and lifting points before raising vehicles
· Review safe systems of work for working underneath vehicles
· Ensure employees remain competent to operate lifting equipment
· Remove defective equipment from service immediately

	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW





	
1. 
	WHAT IS THE HAZARD?
	Vehicle Inspection, Servicing & Repair

	
	Describe what could cause harm
	Injury arising from inspecting, servicing, repairing or maintaining vehicles, including unexpected movement, mechanical components and stored energy

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Cuts, crushing or trapping injuries
· Burns from hot components or fluids
· Injuries from unexpected movement or release of stored energy
· Eye injuries
· Serious injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Vehicles are secured before work begins
· Engines are switched off and keys controlled where appropriate
· Suitable tools and equipment are used for each task
· Employees are trained and competent for the work undertaken
· Manufacturer instructions and safe working procedures are followed
· Hot components and fluids are allowed to cool where necessary
· Defective tools or equipment are removed from use
· Suitable PPE is provided and worn

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review servicing and repair procedures regularly
· Ensure suitable isolation arrangements are used before work begins
· Provide additional training where specialist repairs are undertaken
· Review controls following incidents, near misses or changes to vehicle types



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW



	
1. 
	WHAT IS THE HAZARD?
	Hand Tools & Power Tools

	
	Describe what could cause harm
	Use of hand tools, impact tools, drills, grinders and other portable power tools during vehicle inspection, servicing and repair

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Cuts and lacerations
· Eye injuries from flying particles
· Crushing or trapping injuries
· Burns
· Electric shock
· Hearing damage



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Tools are suitable for the task and used according to manufacturers' instructions
· Employees are appropriately trained and competent
· Tools are inspected and maintained
· Guards and safety features are kept in place
· Damaged or defective tools are removed from use
· Workpieces are secured where necessary
· Suitable PPE is provided and worn
· Tools are stored safely when not in use

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	3
	4
	12 - HIGH



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review tool safety and inspection arrangements
· Ensure employees remain competent to use relevant tools
· Replace or repair defective equipment promptly
· Review PPE and guarding requirements



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM



	
1. 
	WHAT IS THE HAZARD?
	Electrical Systems & Equipment

	
	Describe what could cause harm
	Electrical systems, vehicle electrical components, battery-powered equipment and portable electrical tools used during vehicle repair and maintenance



	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Electric shock
· Electrical burns
· Fire
· Serious or fatal injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Electrical work is carried out by competent persons
· Equipment and tools are inspected and maintained
· Damaged cables, plugs or equipment are removed from use
· Vehicles are isolated from electrical supplies where required
· Suitable tools are used for electrical work
· Employees do not carry out unauthorised electrical repairs
· Electrical defects are reported promptly
· Suitable PPE is provided where required

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review electrical isolation procedures for vehicle and workshop systems
· Ensure employees undertaking specialist electrical work are appropriately competent
· Maintain suitable inspection and maintenance arrangements
· Remove defective equipment from use immediately



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW

	
1. 
	WHAT IS THE HAZARD?
	Batteries & Charging

	
	Describe what could cause harm
	Handling, charging, testing or replacing vehicle batteries, including exposure to electrical energy, battery acid and gases released during charging

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Chemical burns
· Eye injuries
· Electric shock or burns
· Fire or explosion
· Serious injury from short circuits or battery failure



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Batteries are handled by trained and competent employees
· Suitable charging areas are provided where required
· Charging areas are adequately ventilated
· Batteries are secured and handled using suitable equipment
· Suitable PPE is provided, including eye and hand protection
· Smoking and ignition sources are prohibited around charging areas
· Damaged batteries are removed from use and managed safely
· Manufacturer instructions are followed
· Suitable spill control arrangements are available

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review battery charging and storage arrangements
· Ensure suitable ventilation is maintained
· Check employees remain competent to handle and charge batteries
· Review arrangements for damaged or leaking batteries
· Ensure suitable emergency and spill procedures are understood



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW

	
1. 
	WHAT IS THE HAZARD?
	Fuels, Oils & Other Hazardous Substances

	
	Describe what could cause harm
	Handling, storage and use of fuels, oils, lubricants, brake fluids, coolants, solvents, cleaning products and other hazardous substances

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Skin irritation or dermatitis
· Chemical burns
· Eye injuries
· Respiratory irritation
· Ill health following prolonged exposure
· Fire or other harm from flammable substances



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Hazardous substances are identified and assessed where required
· Substances are stored in suitable, labelled containers
· Safety data sheets and relevant product information are available
· Suitable ventilation is provided
· Spill kits are available
· Employees receive appropriate information and instruction
· Suitable PPE is provided and worn
· Flammable substances are kept away from ignition sources
· Waste oils and contaminated materials are disposed of safely

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review COSHH assessments when substances or processes change
· Consider less hazardous alternatives where reasonably practicable
· Review storage and spill arrangements
· Ensure suitable ventilation remains effective
· Consider health surveillance where required

	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	4
	4 - LOW



	1. 
	WHAT IS THE HAZARD?
	Dust, Fumes & Exhaust Emissions

	
	Describe what could cause harm
	Exposure to vehicle exhaust fumes, dust, vapours and other airborne contaminants generated during vehicle repair, maintenance and cleaning activities



	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel
· Visitors



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Eye and respiratory irritation
· Headaches, dizziness or nausea
· Breathing difficulties
· Occupational asthma or other respiratory illness
· Long-term ill health following repeated exposure
· Serious effects from hazardous exhaust gases



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Vehicle engines are not run indoors unnecessarily
· Suitable exhaust extraction is provided where vehicles need to run indoors
· Workshop ventilation is maintained
· Dust and fumes from grinding, sanding or other activities are controlled
· Less hazardous products or processes are used where reasonably practicable
· Employees receive appropriate information and instruction
· Suitable respiratory protective equipment is provided where required
· Extraction systems are maintained and checked appropriately

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	3
	4
	12 - HIGH









	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review workshop ventilation and exhaust extraction arrangements
· Ensure extraction is used whenever required
· Review activities that generate dust, fumes or vapours
· Maintain extraction systems and address defects promptly
· Consider health surveillance where significant exposure cannot otherwise be adequately controlled



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 



	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM






















	
1. 
	WHAT IS THE HAZARD?
	Welding, Grinding & Hot Work

	
	Describe what could cause harm
	Welding, grinding, cutting and other hot work creating sparks, heat, fumes and ignition sources within the garage

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel
· Visitors

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Burns
· Eye injuries
· Exposure to welding fumes
· Fire or explosion
· Serious or fatal injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Hot work is assessed and controlled before work begins
· Flammable materials are removed from the work area
· Suitable screens are used to protect others from sparks and arc flash
· Welding and grinding equipment is maintained and inspected
· Suitable extraction or ventilation is provided
· Gas cylinders are stored and secured appropriately
· Suitable PPE is provided, including eye and face protection
· Suitable firefighting equipment is readily available
· Employees carrying out hot work are appropriately trained

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review hot work arrangements and introduce a permit system where appropriate
· Ensure combustible materials are removed or adequately protected
· Review ventilation and fume extraction arrangements
· Ensure suitable fire precautions are maintained
· Inspect hot work equipment regularly



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW

	
1. 
	WHAT IS THE HAZARD?
	Fire & Explosion

	
	Describe what could cause harm
	Fire or explosion arising from fuels, flammable substances, batteries, hot work, ignition sources or vehicle-related activities

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel
· Visitors

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Burns
· Smoke inhalation
· Serious injury from fire or explosion
· Serious or fatal injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· A suitable fire risk assessment is in place
· Flammable substances are stored safely and away from ignition sources
· Gas cylinders are secured and stored appropriately
· Hot work is controlled
· Smoking and other ignition sources are prohibited in relevant areas
· Suitable fire extinguishers are provided and maintained
· Emergency routes and exits are kept clear
· Employees receive appropriate fire safety information and instruction
· Good housekeeping is maintained to prevent combustible waste accumulating

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review fire risks associated with vehicle repair activities
· Ensure suitable controls are in place for fuels, batteries and hot work
· Review storage arrangements for flammable substances
· Ensure firefighting and emergency arrangements remain suitable
· Reinforce fire procedures where required



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	4
	4 - LOW



	
1. 
	WHAT IS THE HAZARD?
	Noise & Vibration

	
	Describe what could cause harm
	Exposure to excessive noise and vibration from vehicle engines, power tools, compressors, grinders and other workshop equipment

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Hearing damage or tinnitus
· Hand-Arm Vibration Syndrome (HAVS)
· Numbness or reduced grip strength
· Fatigue and reduced concentration
· Long-term ill health



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Noisy and vibrating equipment is identified and assessed
· Lower-noise and lower-vibration equipment is used where reasonably practicable
· Equipment is maintained in good condition
· Exposure times are controlled where appropriate
· Suitable hearing and other protective equipment is provided
· Employees receive appropriate information and instruction
· Health surveillance is provided where required

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	3
	4
	12 - HIGH



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Assess significant noise and vibration exposure
· Review whether alternative equipment or processes could reduce exposure
· Monitor exposure times where necessary
· Review maintenance and PPE arrangements
· Consider health surveillance for regularly exposed employees



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 




	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM

	
1. 
	WHAT IS THE HAZARD?
	Manual Handling

	
	Describe what could cause harm
	Lifting, carrying, pushing, pulling or moving vehicle parts, tyres, tools, equipment and other materials during working activities

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel



	3.  
	WHAT HARM COULD OCCUR? 
	

	
	Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing
	· Back injuries
· Musculoskeletal disorders
· Strains and sprains
· Crush or impact injuries
· Cuts and bruising



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Unnecessary manual handling is avoided where reasonably practicable
· Heavy or awkward items are moved using mechanical aids where appropriate
· Suitable assistance is provided for heavy or bulky items
· Tyre handling equipment is used where appropriate
· Loads are assessed before being moved
· Suitable storage arrangements minimise unnecessary lifting
· Employees receive appropriate information, instruction and training
· Suitable PPE is provided where required

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	3
	3
	9 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review tasks involving heavy, awkward or repetitive handling
· Provide suitable mechanical handling aids where appropriate
· Review storage arrangements to minimise unnecessary handling
· Provide additional training where required



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Site Manager / Site Supervisor
	
	ASSESSOR TO COMPLETE 




	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	3
	6 - MEDIUM

	
1. 
	WHAT IS THE HAZARD?
	Compressed Air & Pressurised Systems

	
	Describe what could cause harm
	Use of compressed air, air tools, compressors, pressurised vehicle systems and other equipment containing stored pressure

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Eye injuries from flying particles
· Injection injuries from compressed air
· Hearing damage
· Burns or impact injuries from equipment failure
· Serious injury following uncontrolled release of pressure



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Compressed air equipment is suitable for its intended use
· Compressors and pressurised systems are maintained and inspected appropriately
· Only suitable hoses, fittings and attachments are used
· Compressed air is not directed at people or used to clean clothing or the body
· Pressure is controlled within safe operating limits
· Defective hoses, connections or equipment are removed from use
· Employees receive appropriate information, instruction and training
· Suitable eye and hearing protection is provided where required

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review compressed air equipment and associated risk assessments
· Ensure pressure systems are appropriately inspected and maintained
· Replace damaged hoses and fittings promptly
· Reinforce safe use of compressed air with employees
· Ensure required examinations of pressure systems are completed

	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	4
	4 - LOW



	
1. 
	WHAT IS THE HAZARD?
	Work at Height & Falling Objects

	
	Describe what could cause harm
	Working above ground level or beneath raised vehicles, equipment or stored items where there is a risk of falling people, tools or materials

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Vehicle repair personnel
· Visitors

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Falls causing fractures or serious injury
· Head injuries
· Cuts and bruising
· Injury from falling tools or vehicle components
· Serious or fatal injury



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Work at height is avoided where reasonably practicable
· Suitable access equipment is used
· Ladders and platforms are inspected and maintained
· Tools and materials are secured when working at height
· Areas below overhead work are controlled where required
· Raised vehicles are secured using suitable supports
· Employees receive appropriate information, instruction and training
· Defective access equipment is removed from use

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	5
	10 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Review work at height activities and access arrangements
· Ensure suitable equipment and fall prevention measures are available
· Prevent tools and materials being left where they could fall
· Review controls following changes to the workshop layout or equipment



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Site Manager / Temporary Works Coordinator / Site Supervisor
	
	ASSESSOR TO COMPLETE 




	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	5
	5 - LOW

	
1. 
	WHAT IS THE HAZARD?
	Housekeeping, Welfare & Emergency Arrangements

	
	Describe what could cause harm
	Poor housekeeping, inadequate welfare facilities or ineffective emergency arrangements within the garage or workshop

	
2. 
	WHO COULD BE HARMED?
	

	
	e.g. employees, contractors, visitors, members of the public etc
	· Employees
· Contractors
· Customers and visitors

	3.  
	WHAT HARM COULD OCCUR? 
	

	
	
Consider the potential consequences, including physical injury, work-related ill health and effects on mental wellbeing

	· Slips, trips and falls
· Ill health from inadequate welfare facilities
· Delayed evacuation during an emergency
· Increased risk of injury during an incident



	4. 
	WHAT ARE YOU ALREADY DOING TO REDUCE THE RISK? 
List the control measures in place 

	
	· Work areas and walkways are kept clear
· Waste and vehicle parts are removed regularly
· Suitable toilets, washing facilities and drinking water are provided
· Emergency routes and exits are kept clear
· First aid equipment is available
· Emergency procedures are communicated to employees
· Suitable fire and emergency equipment is provided and maintained
· Employees are encouraged to report hazards promptly

	5. 
	CURRENT RISK RATING (with existing controls in place) 
Use the risk rating matrix on the front page to score the risk 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	2
	4
	8 - MEDIUM



	6. 
	WHAT ELSE DO YOU NEED TO DO?
Are there any additional control measures needed to reduce the risk further?

	
	· Carry out regular housekeeping and welfare inspections
· Ensure waste and used vehicle parts are removed promptly
· Review emergency arrangements regularly
· Ensure welfare facilities remain suitable for the workforce
· Address any recurring housekeeping or emergency access issues



	7. 
	WHO WILL TAKE ACTION? 
Name or Job role 
	8.
	WHEN SHOULD THIS BE COMPLETED?
Target date

	
	Garage Manager / Workshop Supervisor
	
	ASSESSOR TO COMPLETE 


	9. 
	RISK RATING AFTER ACTION (expected risk once action completed) 

	
	Likelihood (L)
	Severity (S)
	Risk (L x S = R) 

	
	1
	4
	4 - LOW




RISK ASSESSMENT: Review & Sign-off

	YOUR ACTION PLAN

	OUTSTANDING ACTION
	RESPONSIBLE PERSON
	TARGET DATE
	COMPLETED

	

	
	
	

	

	
	
	

	

	
	
	

	

	
	
	

	

	
	
	


COMMUNICATION
Relevant findings and control measures from this assessment must be communicated to employees and others who may be affected.  
REVIEW THIS ASSESSMENT
This risk assessment should be reviewed if there is reason to believe it is no longer valid or following significant change to the work, workplace, equipment, processes or people affected. 

Next planned review date: 

	ASSESSMENT COMPLETED BY
	APPROVED/REVIEWED BY (if applicable)

	Name: 
	Name: 

	Position: 
	Position: 

	Signature: 
	Signature: 

	Date: 
	Date: 
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